Package pygeodesy :: Module rhumbx :: Class RhumbLine |
[frames] | no frames]

# Class RhumbLine

      object --+
               |
    named._Named --+
                   |
    named._NamedBase --+
                       |
        karney._CapsBase --+
                           |
         rhumbBase.RhumbBase --+
                               |
         rhumbBase.RhumbLineBase --+
                                   |
                                  RhumbLine

Compute one or several points on a single rhumb line.

Class `RhumbLine` facilitates the determination of points on a single rhumb line. The starting point (`lat1`, `lon1`) and the azimuth `azi12` are specified once.

Method `RhumbLine.Position` returns the location of an other point at distance `s12` along and the area `S12` under the rhumb line.

Method `RhumbLine.intersection2` finds the intersection between two rhumb lines.

Method `RhumbLine.nearestOn4` computes the nearest point on and the distance to a rhumb line in different ways.

Instance Methods
__init__(self, rhumb, lat1=0, lon1=0, azi12=None, **caps_name) New `rhumbx.RhumbLine`. |
Position(self, s12, outmask=384) Compute a point at a given distance on this rhumb line. |
Inherited from `rhumbBase.RhumbLineBase`: `__del__`, `distance2`, `intersection2`, `nearestOn4`, `toStr` Inherited from `rhumbBase.RhumbBase`: `Direct`, `Direct8`, `DirectLine`, `Inverse`, `Inverse8`, `InverseLine`, `Line` Inherited from `karney._CapsBase`: `caps_` Inherited from `named._NamedBase`: `__repr__`, `__str__`, `others`, `toRepr` Inherited from `named._Named`: `__imatmul__`, `__matmul__`, `__rmatmul__`, `attrs`, `classof`, `copy`, `dup`, `methodname`, `rename`, `toStr2` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Class Variables
Inherited from `karney._CapsBase`: `ALL`, `AREA`, `AZIMUTH`, `DISTANCE`, `DISTANCE_IN`, `EMPTY`, `GEODESICSCALE`, `LATITUDE`, `LINE_OFF`, `LONGITUDE`, `LONG_UNROLL`, `REDUCEDLENGTH`, `STANDARD`

Properties
| RAorder Get this rhumb line's Rhumb Area order (`int`, 4, 5, 6, 7 or 8).
Inherited from `rhumbBase.RhumbLineBase`: `TMorder`, `azi12`, `azi12_sincos2`, `ellipsoid`, `exact`, `isLoxodrome`, `lat1`, `latlon1`, `lon1`, `rhumb`, `xTM` Inherited from `rhumbBase.RhumbBase`: `a`, `b`, `equatoradius`, `f`, `f_max`, `flattening`, `polaradius` Inherited from `karney._CapsBase`: `caps`, `debug` Inherited from `named._Named`: `classname`, `classnaming`, `iteration`, `name`, `named`, `named2`, `named3`, `named4`, `sizeof` Inherited from `object`: `__class__`

Method Details

### __init__ (self, rhumb, lat1=0, lon1=0, azi12=None, **caps_name) (Constructor) |
New `rhumbx.RhumbLine`. Arguments: `rhumb` - The rhumb reference (`rhumbx.Rhumb`). `lat1` - Latitude of the start point (`degrees90`). `lon1` - Longitude of the start point (`degrees180`). `azi12` - Azimuth of this rhumb line (compass `degrees`). `caps_name` - Optional keyword arguments `name=NN` and `caps=0`, a bit-or'ed combination of Caps values specifying the required capabilities. Include `Caps.LINE_OFF` if updates to the `rhumb` should not be reflected in this rhumb line. Overrides: object.__init__

### Position (self, s12, outmask=384) |
Compute a point at a given distance on this rhumb line. Arguments: `s12` - The distance along this rhumb between its point and the other point (`meters`), can be negative. `outmask` - Bit-or'ed combination of Caps values specifying the quantities to be returned. Returns: GDict with 4 to 8 items `azi12, a12, s12, S12, lat2, lon2, lat1, lon1` with latitude `lat2` and longitude `lon2` of the point in `degrees`, the rhumb angle `a12` in `degrees` from the start point of and the area `S12` under this rhumb line in `meter` squared. Overrides: rhumbBase.RhumbLineBase.Position Note: If `s12` is large enough that the rhumb line crosses a pole, the longitude of the second point is indeterminate and `NAN` is returned for `lon2` and area `S12`. If the first point is a pole, the cosine of its latitude is taken to be `sqrt(EPS)`. This position is extremely close to the actual pole and allows the calculation to be carried out in finite terms.

Property Details

### RAorder Get this rhumb line's Rhumb Area order (`int`, 4, 5, 6, 7 or 8). Get method: RAorder(self) - Get this rhumb line's Rhumb Area order (`int`, 4, 5, 6, 7 or 8). Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst) - Zap the cached/memoized `property` value.